Guide for cutting Electronic/Chip car keys

1. Insert original key in the “RW4\*” key programming machine
2. Select “Copy” on the main menu
3. Press the “Rd” key when prompted
4. Choose one of the following options depending on the response from the key machine
   1. If the key machine says “Insert Blank Key”
      1. Then look up the required key for the car
      2. Tell the customer the price of the key and confirm whether they are still interested in the key (Also verify all required parts are in stock)
      3. Remove the original key from the programming machine
      4. Insert the new blank head or entire key
      5. Press the “Wr” button to program the key
   2. If the key machine says “Key Data Processing”
      1. Wait for the key machine to finishing processing the data
      2. If it says “Insert Blank Key” after processing then follow option (a.)
      3. If it says “Transponder Cannot Duplicate” then the customer must get the key from the dealer or another vendor
   3. If the key machine says “Insert snoop”
      1. Then look up the required key for the car
      2. Tell the customer the price of the key and confirm whether they are still interested in the key (Also verify all required parts are in stock)
      3. Ask the customer if they have the vehicle that the key operates with them and proceed if they do if they don’t ask them to come back with the vehicle as it is required to make this key
      4. Insert the antenna end of the “Snoop” into the port on the key machine where you would normally insert a key (The antenna end of the Snoop is the smallest end and has an elastic band that is attached to it)
      5. Press the “Enter” key on the programming machine
      6. Take the “Snoop” to the vehicle and put the elastic band around the head of the original key
      7. Insert the original key into the vehicles ignition with the antenna attached to the key head
      8. Turn the vehicle on and off until (do not turn it off and on too rapidly) the 2 lights on the snoop become solid
      9. Once both lights on the snoop are solid proceed back to the programmer
      10. Insert the snoop antenna in the programmer and press “Enter”
      11. Take the snoop out of the programmer
      12. Insert the original key into the programmer again and press “Enter”
      13. Wait for the key machine to finishing processing
      14. Insert the blank key head (Usually item # “EH3P” not “EH3”) and press “Wr”
5. Upon successful completion of the programming cut the new key blank
6. Go to the customers vehicle and test the key or if vehicle is not present ask the customer to verify the key works when they can